Headline
*  testcase large Cp        *
Lwl            Length of waterline
   73.0
Lwl / Bwl      Ratio of waterline length to waterline beam
   7.09
Bwl / Tcb      Ratio of waterline beam to Draft of canoe body
   3.29
Beck / Bwl     Ratio of beam at decklevel to waterline beam
   1.0
Cp             Prismatic coefficient of c.b.
   0.85
Cm             Coefficient of the maximum area section
   0.85
LCB/Lwl        Longitudinal center of buoyancy, distance from fpp divided by Lwl
   0.5
LCF/Lwl        Longitudinal center of flotation, distance from fpp divided by Lwl
   0.51
Awl / Vol^2/3  Ratio of waterplane area to the 2/3rd power of the volume
   4.8
Alpha          Flare angle at max. area section, DWL-level, degrees outward from vertical
   1.
Gamma          Deadrise angle at the keel, in degrees upward from horizontal
   0.0                                       combine larger values with U_SEC = 0.
D / Lwl        Ratio of depth of canoe body to Lwl
   0.0877
TOH / Lwl      Ratio of transom overhang to Lwl in percent
   1.
TCL / TOH      Ratio of transom clearance to transom overhang
  999                                             if unknown use default 999
TRANSOM        Parameter for transom size, see user manual, or use = 1.
   4.
U_SEC          Parameter describing radius of U-sections in forebody
   0.                                             = 0. for V-sections
BOW_FLAR       Parameter causing additional flare at bow if > 0
   0.1
CADOUT         specifies the output file. 1=Rhino, 2=DelftShip, 3=ProSurf, 4=UliTank
   2
*** the following lines can be used for comments **
