Headline
*  Delft Series parent model Sysser 25       *
Lwl            Length of waterline
   10.0
Lwl / Bwl      Ratio of waterline length to waterline beam
   4.0
Bwl / Tcb      Ratio of waterline beam to Draft of canoe body
   5.388
Bdeck / Bwl    Ratio of beam at decklevel to waterline beam
   1.12
Cp             Prismatic coefficient of c.b.
   0.5483
Cm             Coefficient of the maximum area section
   0.727
LCB/Lwl        Longitudinal center of buoyancy, distance from fpp divided by Lwl
   0.5199
LCF/Lwl        Longitudinal center of flotation, distance from fpp divided by Lwl
   0.5554
Awl / Vol^2/3  Ratio of waterplane area to the 2/3rd power of the volume
   6.048
Alpha          Flare angle at max. area section, DWL-level, degrees outward from vertical
   32.5
Gamma          Deadrise angle at the keel, in degrees upward from horizontal
   0.0                                       combine larger values with U_SEC = 0.
D / Lwl        Ratio of depth of canoe body to Lwl
   0.13463
TOH / Lwl      Ratio of transom overhang to Lwl in percent
  20.0
TCL / TOH      Ratio of transom clearance to transom overhang
  0.141                                           if unknown use default 999
TRANSOM        Parameter for transom size, see user manual, or use = 1.
   3.
U_SEC          Parameter describing radius of U-sections in forebody
   3.                                             = 0. for V-sections
BOW_FLAR       Parameter causing additional flare at bow if > 0
   0.
CADOUT         specifies the output file. 1=Rhino, 2=DelftShip, 3=ProSurf, 4=UliTank
   1
*** the following lines can be used for comments **
