*  keel Dehler 33  *
   ACOFFK section area coefficient
     0.648
   TFIN   draft of fin-keel from root (highest point) to tip, at right angle to waterplane (m)
     1.6
   SWEEP  sweep angle of fin-keel at 1/4-cord-line in degrees
     10.0
   Chord (m), thickness ratio, for the given vertical position
   0.8868     0.1224           at fin-root, close to canoe body
   0.8868     0.1224           at 19.51% TFIN down from root
   0.8868     0.1183           at 38.27% TFIN down from root
   0.8868     0.1171           at 55.56% TFIN down from root
   0.8868     0.1210           at 70.71% TFIN down from root
   0.931      0.1252           at 83.15% TFIN down from root
   1.2042     0.1384           at 92.39% TFIN down from root
   1.2312     0.1563           at 98.08% TFIN down from root
   KSTYPE  keel foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     64
   BULBL lenght in (m) of additional ballast bulb at tip of fin, without bulb type 0.
      0.
   BULBW width of ballast bulb in (m)
      0.
   BULBH height of ballast bulb in (m)
      0.
*  rudder Dehler 33           *
   DYRUD for twin rudders = y-distance of root from centerline in (m), for one rudder = 0.
      0.
   INCLIN for twin rudders = inclination to vertical in (deg.), for one rudder = 0.
      0.
   CRUDU  chord length at upper end of LE, parallel to the waterplane (m)
     0.512 
   CRUDL  chord length at lower end of TE, parallel to the waterplane (m)
     0.223  
   TRUD   rudder span along the blade, at right angle to centerline from CRUDU to CRUDL (m)
     1.366
   SWEEPR  sweep angle of 1/4 point line relative to the line that defines TRUD, in degrees
     20.2
   TCRDU  thicknes ratio of upper section at top (-)
     0.16
   TCRDL  thicknes ratio of lower section at tip (-)
     0.11
   ACOFFR section area coefficient
     0.6648
   RSTYPE  rudder foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     64
