*  keel H-Boat  *
   ACOFFK section area coefficient
     0.703
   TFIN   draft of fin-keel from root (highest point) to tip, at right angle to waterplane (m)
     0.833
   SWEEP  sweep angle of fin-keel at 1/4-cord-line in degrees
     48.4
   Chord (m), thickness ratio, for the given vertical position
   1.8902     0.0815           at fin-root, tangential to deepest point of canoe body
   1.5284     0.0981           at 19.51% TFIN down from root
   1.3817     0.1086           at 38.27% TFIN down from root
   1.2891     0.1254           at 55.56% TFIN down from root
   1.2081     0.1487           at 70.71% TFIN down from root
   1.1415     0.1577           at 83.15% TFIN down from root
   1.0921     0.1685           at 92.39% TFIN down from root
   0.8944     0.1894           at 98.08% TFIN down from root
   KSTYPE  keel foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     64
   BULBL lenght in (m) of additional ballast bulb at tip of fin, without bulb type 0.
      0.
   BULBW width of ballast bulb in (m)
      0.
   BULBH height of ballast bulb in (m)
      0.
*  rudder H-boat       *
   DYRUD for twin rudders = y-distance of root from centerline in (m), for one rudder = 0.
      0.
   INCLIN for twin rudders = inclination to vertical in (deg.), for one rudder = 0.
      0.
   CRUDU  chord length at upper end of LE, parallel to the waterplane (m)
     0.519 
   CRUDL  chord length at lower end of TE, parallel to the waterplane (m)
     0.276  
   TRUD   rudder span along the blade, at right angle to centerline from CRUDU to CRUDL (m)
     1.04
   SWEEPR  sweep angle of 1/4 point line relative to the line that defines TRUD, in degrees
     24.
   TCRDU  thicknes ratio of upper section at top (-)
     0.114
   TCRDL  thicknes ratio of lower section at tip (-)
     0.114
   ACOFFR section area coefficient
     0.63
   RSTYPE  rudder foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     63
