*  keel Class 40  *
   ACOFFK section area coefficient
     0.648
   TFIN   draft of fin-keel from root (highest point) to tip, at right angle to waterplane (m)
     2.342
   SWEEP  sweep angle of fin-keel at 1/4-cord-line in degrees
     0.0
   Chord (m), thickness ratio, for the given vertical position
   0.6772      0.13           at fin-root, tangential to deepest point of canoe body
   0.6472      0.13           at 19.51% TFIN down from root
   0.6183      0.13           at 38.27% TFIN down from root
   0.5917      0.13           at 55.56% TFIN down from root
   0.5684      0.13           at 70.71% TFIN down from root
   0.5492      0.13           at 83.15% TFIN down from root
   0.5350      0.13           at 92.39% TFIN down from root
   0.5263      0.13           at 98.08% TFIN down from root
   KSTYPE  keel foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     64
   BULBL lenght in (m) of additional ballast bulb at tip of fin, without bulb type 0.
      2.46
   BULBW width of ballast bulb in (m)
      0.523
   BULBH height of ballast bulb in (m)
      0.307
*  rudder Class 40           *
   DYRUD for twin rudders = y-distance of root from centerline in (m), for one rudder = 0.
     1.3
   INCLIN for twin rudders = inclination to vertical in (deg.), for one rudder = 0.
     14.4
   CRUDU  chord length at upper end of LE, parallel to the waterplane (m)
     0.43 
   CRUDL  chord length at lower end of TE, parallel to the waterplane (m)
     0.154  
   TRUD   rudder span along the blade, at right angle to centerline from CRUDU to CRUDL (m)
     1.363
   SWEEPR  sweep angle 1/4-cord-line of rudder relative to vertical on centerline in degrees
     0.
   TCRDU  thicknes ratio of upper section at top (-)
     0.14
   TCRDL  thicknes ratio of lower section at tip (-)
     0.14
   ACOFFR section area coefficient
     0.6648
   RSTYPE  rudder foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     64
