*  keel v01, all dimensions full scale  *
   ACOFFK section area coefficient
     0.648
   TFIN   draft of fin-keel from root (highest point) to tip, at right angle to waterplane (m)
     0.327
   SWEEP  sweep angle of fin-keel at 1/4-cord-line in degrees
     0.0
   Chord (m), thickness ratio, for the given vertical position
   0.0800     0.122           at fin-root, tangential to deepest point of canoe body
   0.0800     0.122           at 19.51% TFIN down from root
   0.0800     0.122           at 38.27% TFIN down from root
   0.0800     0.122           at 55.56% TFIN down from root
   0.0800     0.122           at 70.71% TFIN down from root
   0.0800     0.122           at 83.15% TFIN down from root
   0.0800     0.122           at 92.39% TFIN down from root
   0.0800     0.122           at 98.08% TFIN down from root
   KSTYPE  keel foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     64
   BULBL lenght in (m) of additional ballast bulb at tip of fin, without bulb type 0.
     0.380
   BULBW width of ballast bulb in (m)
     0.036
   BULBH height of ballast bulb in (m)
     0.036
*  rudder v01           *
   DYRUD for twin rudders = y-distance of root from centerline in (m), for one rudder = 0.
     0.
   INCLIN for twin rudders = inclination to vertical in (deg.), for one rudder = 0.
     0.
   CRUDU  chord length at upper end of LE, parallel to the waterplane (m)
     0.070 
   CRUDL  chord length at lower end of TE, parallel to the waterplane (m)
     0.050  
   TRUD   rudder span along the blade, at right angle to centerline from CRUDU to CRUDL (m)
     0.190
   SWEEPR  sweep angle of 1/4 point line relative to the line that defines TRUD, in degrees
     10.0
   TCRDU  thicknes ratio of upper section at top (-)
      0.16
   TCRDL  thicknes ratio of lower section at tip (-)
      0.011
   ACOFFR section area coefficient
     0.6648
   RSTYPE  rudder foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     64
