
*    USSAIL #M5   *                                                   
 Geometry defined in: OFFS_us5.TXT
 
 Hull properties calculated with UliTank 3.3
 for details see www.remmlinger.com
 
 values upright at rest, without trim in fresh water
 immersed volume canoe body (m3) =   1.11663   
 immersed volume fin keel (m3)   =   0.46451E-1
 immersed volume rudder (m3)     =   0.64591E-2
 total mass of the yacht (kg)    =    1168.3   
 wetted surface canoe body (m2)  =   7.47892   
 waterplane area (m2)            =   6.74128   
 waterline length (m)            =    6.215
 maximum beam in waterplane (m)  =    1.572
 maximum draft canoe body (m)    =    0.279
 maximum draft with keel (m)     =    1.501
 Cx                              =   0.7642
 Cp                              =   0.5429
 Cwp                             =   0.6899
 LCB in % Lwl behind FP          =   54.704
 LCF in % Lwl behind FP          =   57.479
 Rocker angle aft end DWL (deg)  =   10.235
