*  Standard keel USSAIL#5, all dimensions at tank model scale  *
   DXCOGK distance COG to LE keel (m)
     0.8134
   ACOFFK section area coefficient of keel-foil
     0.657
   TFIN   draft of fin-keel from root (lowest point) to tip, at right angle to waterplane (m)
     2.443
   SWEEP  sweep angle of fin-keel at 1/4-cord-line in degrees
     9.2
   Chord (m), thickness ratio, for the given vertical position
   1.585      0.1306           at fin-root, close to canoe body
   1.4818     0.1306           at 19.51% TFIN down from root
   1.38256    0.1306           at 38.27% TFIN down from root
   1.2911     0.1306           at 55.56% TFIN down from root
   1.21094    0.1306           at 70.71% TFIN down from root
   1.14515    0.1306           at 83.15% TFIN down from root
   1.09627    0.1306           at 92.39% TFIN down from root
   1.06616    0.1306           at 98.08% TFIN down from root
   KSTYPE  keel foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     64
*  Standard rudder USSAIL#5           *
   DXCOGR distance COG to LE rudder (m)
     0.5416
   TRUD   draft of rudder from DWL (as defined by ZDWL) to  aft edge of tip, at right angle to waterplane (m)
     2.211
   SWEEPR  sweep angle of rudder at 1/4-cord-line relative to waterplane in degrees
     15.85
   CURUD  upper chord at waterplane-level (m), if necessary extended inside the cb to the LE
     0.715 
   CLRUD  lower chord at tip (m), parallel to waterplane
     0.341  
   TCURD  thicknes ratio of upper section at top (-)
     0.1272
   TCLRD  thicknes ratio of lower section at tip (-)
     0.1272
   ACOFFR section area coefficient of rudder-foil
     0.6625
   RSTYPE  rudder foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     64
