
* monohull of catamaran Delft 372 - format "stations" from DelftShip  
 Geometry defined in: OFFS_dsh.TXT
 
 Hull properties calculated with UliTank 3.3
 for details see www.remmlinger.com
 
 values upright at rest, without trim in fresh water
 immersed volume canoe body (m3) =  0.435600E-1
 total mass of the yacht (kg)    =    43.517   
 wetted surface canoe body (m2)  =  0.966719   
 waterplane area (m2)            =  0.545575   
 waterline length (m)            =    3.000
 maximum beam in waterplane (m)  =    0.233
 maximum draft canoe body (m)    =    0.150
 Cx                              =   0.6858
 Cp                              =   0.6168
 Cwp                             =   0.7802
 LCB in % Lwl behind FP          =   52.614
 LCF in % Lwl behind FP          =   58.237
 Rocker angle aft end DWL (deg)  =    9.658
