*  Standard keel DSYHS, all dimensions at tank model scale  *
   DXCOGK distance COG to LE keel (m)
     0.2582
   ACOFFK section area coefficient
     0.6581
   TFIN   draft of fin-keel from root (highest point) to tip, at right angle to waterplane (m)
     0.219
   SWEEP  sweep angle of fin-keel at 1/4-cord-line in degrees
     45.0
   Chord (m), thickness ratio, for the given vertical position
   0.4140     0.15             at fin-root, close to canoe body
   0.3843     0.15             at 19.51% TFIN down from root
   0.3558     0.15             at 38.27% TFIN down from root
   0.3295     0.15             at 55.56% TFIN down from root
   0.3065     0.15             at 70.71% TFIN down from root
   0.2876     0.15             at 83.15% TFIN down from root
   0.2736     0.15             at 92.39% TFIN down from root
   0.2649     0.15             at 98.08% TFIN down from root
   KSTYPE  keel foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     63
*  Standard rudder DSYHS           *
   DXCOGR distance COG to LE rudder (m)
     0.0613
   TRUD   draft of rudder from DWL (as defined by ZDWL) to tip, at right angle to waterplane (m)
     0.266
   SWEEPR  sweep angle of rudder at 1/4-cord-line relative to waterplane in degrees
     5.5
   CURUD  upper chord at waterplane-level (m), if necessary extended inside the cb to the LE
     0.124 
   CLRUD  lower chord at tip (m), parallel to waterplane
     0.096  
   TCURD  thicknes ratio of upper section at top (-)
      0.1193
   TCLRD  thicknes ratio of lower section at tip (-)
      0.1193
   ACOFFR section area coefficient
     0.6786
   RSTYPE  rudder foil section type: 63 = NACA 63(2)A015, 64 = NACA 64(2)A013, 00 = NACA0012
     00
