
*    USSAIL #M6 full size  *                                          
 Geometry defined in: OFFS_us6.TXT
 
 Hull properties calculated with UliTank 3.3
 for details see www.remmlinger.com
 
 values upright at rest, without trim in seawater
 immersed volume canoe body (m3) =   8.68480   
 immersed volume fin keel (m3)   =   0.37151   
 immersed volume rudder (m3)     =   0.51892E-1
 total mass of the yacht (kg)    =    9344.0   
 wetted surface canoe body (m2)  =   32.4066   
 waterplane area (m2)            =   30.3556   
 waterline length (m)            =   12.343
 maximum beam in waterplane (m)  =    3.574
 maximum draft canoe body (m)    =    0.483
 maximum draft with keel (m)     =    2.926
 Cx                              =   0.7669
 Cp                              =   0.5452
 Cwp                             =   0.6964
 LCB in % Lwl behind FP          =   54.639
 LCF in % Lwl behind FP          =   57.358
 Rocker angle aft end DWL (deg)  =    8.882
