
*    Class 40 - full size   *                                         
 Geometry defined in: OFFS_c40.TXT
 
 Hull properties calculated with UliTank 3.3
 for details see www.remmlinger.com
 
 values upright at rest, without trim in fresh water
 immersed volume canoe body (m3) =   4.81179   
 total mass of the yacht (kg)    =    4803.9   
 wetted surface canoe body (m2)  =   33.1533   
 waterplane area (m2)            =   32.5198   
 waterline length (m)            =   12.130
 maximum beam in waterplane (m)  =    3.901
 maximum draft canoe body (m)    =    0.246
 Cx                              =   0.7214
 Cp                              =   0.5731
 Cwp                             =   0.6875
 LCB in % Lwl behind FP          =   55.698
 LCF in % Lwl behind FP          =   58.101
 Rocker angle aft end DWL (deg)  =    5.522
