
*    DSYHS Sysser 72 - GHS-offset-file from ProSurf  *                
 Geometry defined in: OFFS_ghs.TXT
 
 Hull properties calculated with UliTank 3.3
 for details see www.remmlinger.com
 
 values upright at rest, without trim in fresh water
 immersed volume canoe body (m3) =  0.161120E-1
 total mass of the yacht (kg)    =    16.087   
 wetted surface canoe body (m2)  =  0.499124   
 waterplane area (m2)            =  0.438511   
 waterline length (m)            =    2.008
 maximum beam in waterplane (m)  =    0.342
 maximum draft canoe body (m)    =    0.060
 Cx                              =   0.7650
 Cp                              =   0.5181
 Cwp                             =   0.6420
 LCB in % Lwl behind FP          =   55.952
 LCF in % Lwl behind FP          =   57.972
 Rocker angle aft end DWL (deg)  =    5.273
