
*    Wide-Light-Project   *                                           
 Geometry defined in: OFFS_wlp.TXT
 
 Hull properties calculated with UliTank 3.3
 for details see www.remmlinger.com
 
 values upright at rest, without trim in fresh water
 immersed volume canoe body (m3) =  0.197237   
 total mass of the yacht (kg)    =    196.93   
 wetted surface canoe body (m2)  =   3.26357   
 waterplane area (m2)            =   3.07889   
 waterline length (m)            =    4.721
 maximum beam in waterplane (m)  =    0.877
 maximum draft canoe body (m)    =    0.108
 Cx                              =   0.7986
 Cp                              =   0.5637
 Cwp                             =   0.7437
 LCB in % Lwl behind FP          =   52.414
 LCF in % Lwl behind FP          =   56.803
 Rocker angle aft end DWL (deg)  =    4.244
